IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2020-12-23T14:23:33"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190510_1515(x64) - Exporter 18.4.0.0 - Alternate UI 18.4.0.0"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "ktemmerman" of Organization (no name given)
  Owner history of Person "ktemmerman" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 1608728402 (2020-12-23T13:00:02Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 63 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall_Recticel Insulation:95064" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall_Recticel Insulation" 10.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          16 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "standard" | object type "BERSfr_XX_GM_FB_logo_recticel:standard" | names: "BERSfr_XX_GM_FB_logo_recticel:standard:95087", "BERSfr_XX_GM_FB_logo_recticel:standard:95106", "BERSfr_XX_GM_FB_logo_recticel:standard:95125" (+13 more) | material: materials ("BERSnl_x_rgb 0 0 0 T00 noir_gen", "RSen_x_rgb 255 203 012 T00 yellow_gen") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          31 x IFCBUILDINGELEMENTPROXY | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:95090", "Model Text:Model Text 1:95108", "Model Text:Model Text 1:95109" (+28 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x100_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x100_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x100_Recticel Insulation:95091" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x100_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x100_Recticel Insulation" 100.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x110_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x110_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x110_Recticel Insulation:95110" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x110_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x110_Recticel Insulation" 110.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x120_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x120_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x120_Recticel Insulation:95129" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x120_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x120_Recticel Insulation" 120.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x130_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x130_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x130_Recticel Insulation:95148" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x130_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x130_Recticel Insulation" 130.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x140_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x140_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x140_Recticel Insulation:95167" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x140_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x140_Recticel Insulation" 140.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x150_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x150_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x150_Recticel Insulation:95186" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x150_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x150_Recticel Insulation" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x160_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x160_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x160_Recticel Insulation:95205" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x160_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x160_Recticel Insulation" 160.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x180_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x180_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x180_Recticel Insulation:95224" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x180_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x180_Recticel Insulation" 180.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x30_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x30_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x30_Recticel Insulation:95243" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x30_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x30_Recticel Insulation" 30.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x40_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x40_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x40_Recticel Insulation:95262" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x40_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x40_Recticel Insulation" 40.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x50_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x50_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x50_Recticel Insulation:95281" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x50_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x50_Recticel Insulation" 50.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x60_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x60_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x60_Recticel Insulation:95300" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x60_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x60_Recticel Insulation" 60.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x70_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x70_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x70_Recticel Insulation:95319" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x70_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x70_Recticel Insulation" 70.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x82_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x82_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x82_Recticel Insulation:95338" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x82_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x82_Recticel Insulation" 82.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x95_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x95_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x95_Recticel Insulation:95357" | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x95_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x95_Recticel Insulation" 95.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon

Types
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall_Recticel Insulation" 10.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "standard" | 16 occurrences | material: materials ("BERSnl_x_rgb 0 0 0 T00 noir_gen", "RSen_x_rgb 255 203 012 T00 yellow_gen") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x100_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x100_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x100_Recticel Insulation" 100.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x110_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x110_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x110_Recticel Insulation" 110.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x120_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x120_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x120_Recticel Insulation" 120.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x130_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x130_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x130_Recticel Insulation" 130.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x140_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x140_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x140_Recticel Insulation" 140.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x150_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x150_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x150_Recticel Insulation" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x160_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x160_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x160_Recticel Insulation" 160.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x180_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x180_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x180_Recticel Insulation" 180.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x30_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x30_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x30_Recticel Insulation" 30.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x40_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x40_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x40_Recticel Insulation" 40.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x50_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x50_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x50_Recticel Insulation" 50.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x60_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x60_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x60_Recticel Insulation" 60.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x70_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x70_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x70_Recticel Insulation" 70.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x82_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x82_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x82_Recticel Insulation" 82.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x95_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurowall 1200x600x95_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurowall 1200x600x95_Recticel Insulation" 95.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon

Property sets
  Pset_ElementShading | properties | on 16 objects (16 IFCWALLSTANDARDCASE) | on 16 type objects
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProductRequirements | properties | on 47 objects (47 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 16 objects (16 IFCWALLSTANDARDCASE) | on 16 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 31 objects (31 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 16 objects (16 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "standard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall 1200x600x110_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall 1200x600x130_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall 1200x600x140_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 10 more contents on 10 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall 1200x600x100_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall 1200x600x110_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall 1200x600x120_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall 1200x600x130_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall 1200x600x140_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall 1200x600x150_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurowall 1200x600x160_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 8 more contents on 8 objects not shown
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurowall_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 2.2 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurowall 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.22 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurowall 1200x600x110_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.2 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurowall 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.183333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurowall 1200x600x130_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.169230769230769 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurowall 1200x600x140_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.157142857142857 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurowall 1200x600x150_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.146666666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurowall 1200x600x160_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.1375 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon: 24 more contents on 8 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 31 objects (31 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 16 objects (16 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "standard" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)

Other addresses and roles
  2 x postal address (none given)