IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2020-12-23T14:15:57"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190510_1515(x64) - Exporter 18.4.0.0 - Alternate UI 18.4.0.0"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "ktemmerman" of Organization (no name given)
  Owner history of Person "ktemmerman" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 1608728403 (2020-12-23T13:00:03Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 47 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Powerwall_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Powerwall_Recticel Insulation:76186" | material: layers "Basic Wall:BERSnl_22_WA_Powerwall_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall_Recticel Insulation" 10.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          12 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "standaard" | object type "BERSnl_XX_GM_FB_logo_recticel:standaard" | names: "BERSnl_XX_GM_FB_logo_recticel:standaard:76201", "BERSnl_XX_GM_FB_logo_recticel:standaard:76220", "BERSnl_XX_GM_FB_logo_recticel:standaard:76239" (+9 more) | material: materials ("BERSnl_x_rgb 0 0 0 T00 zwart_gen", "BERSnl_x_rgb 255 203 012 T00 geel_gen") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Other
          23 x IFCBUILDINGELEMENTPROXY | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:76204", "Model Text:Model Text 1:76222", "Model Text:Model Text 1:76223" (+20 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation:76205" | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x100_Recticel Insulation" 100.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation:76224" | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x120_Recticel Insulation" 120.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation:76243" | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x140_Recticel Insulation" 140.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation:76262" | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x160_Recticel Insulation" 160.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x180_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x180_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x180_Recticel Insulation:76281" | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x180_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x180_Recticel Insulation" 180.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x40_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x40_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x40_Recticel Insulation:76300" | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x40_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x40_Recticel Insulation" 40.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x50_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x50_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x50_Recticel Insulation:76319" | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x50_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x50_Recticel Insulation" 50.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x60_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x60_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x60_Recticel Insulation:76338" | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x60_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x60_Recticel Insulation" 60.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x70_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x70_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x70_Recticel Insulation:76357" | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x70_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x70_Recticel Insulation" 70.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x80_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x80_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x80_Recticel Insulation:76376" | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x80_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x80_Recticel Insulation" 80.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x90_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x90_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x90_Recticel Insulation:76395" | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x90_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x90_Recticel Insulation" 90.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading

Types
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Powerwall_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall_Recticel Insulation" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "standaard" | 12 occurrences | material: materials ("BERSnl_x_rgb 0 0 0 T00 zwart_gen", "BERSnl_x_rgb 255 203 012 T00 geel_gen") | property sets: Constraints, Identity Data, Materials and Finishes, Other, Pset_BuildingElementProxyCommon, Pset_ProductRequirements
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x100_Recticel Insulation" 100.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x120_Recticel Insulation" 120.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x140_Recticel Insulation" 140.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x160_Recticel Insulation" 160.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x180_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x180_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x180_Recticel Insulation" 180.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x40_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x40_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x40_Recticel Insulation" 40.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x50_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x50_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x50_Recticel Insulation" 50.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x60_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x60_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x60_Recticel Insulation" 60.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x70_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x70_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x70_Recticel Insulation" 70.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x80_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x80_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x80_Recticel Insulation" 80.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x90_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Powerwall 1200x600x90_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Powerwall 1200x600x90_Recticel Insulation" 90.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading

Property sets
  Other(Type) | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Model Text" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Work Plane = "Level : Level 1" (IFCTEXT)
  Constraints | properties | on 12 objects (12 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 4000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : BERSnl_22_WA_Powerwall_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : BERSnl_22_WA_Powerwall 1200x600x180_Recticel Insulation" (IFCTEXT)
  Constraints: 8 more contents on 7 objects not shown
  Dimensions | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Depth = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY)
    Area = 0.114476516316835 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.000206579980456013 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.134111999999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.34112000000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.60934400000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.87756800000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 2.14579200000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 2.414016 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 7 more contents on 7 objects not shown
  Other | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Model Text: Model Text 1" (IFCLABEL)
    Family and Type = "Model Text: Model Text 1" (IFCLABEL)
    Type = "Model Text: Model Text 1" (IFCLABEL)
    Type Id = "Model Text: Model Text 1" (IFCLABEL)
  Other | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "BERSnl_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Family and Type = "BERSnl_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Type = "BERSnl_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Type Id = "BERSnl_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: BERSnl_22_WA_Powerwall_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: BERSnl_22_WA_Powerwall_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: BERSnl_22_WA_Powerwall_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: BERSnl_22_WA_Powerwall_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" (IFCLABEL)
  Other: 10 more contents on 8 objects not shown
  Phasing | properties | on 47 objects (35 IFCBUILDINGELEMENTPROXY, 12 IFCWALLSTANDARDCASE)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 12 objects (12 IFCWALLSTANDARDCASE)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 12 objects (12 IFCWALLSTANDARDCASE) | on 12 type objects
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProductRequirements | properties | on 35 objects (35 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 12 objects (12 IFCWALLSTANDARDCASE) | on 12 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "standaard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall 1200x600x180_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 6 more contents on 6 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall 1200x600x180_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall 1200x600x40_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Powerwall 1200x600x50_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 4 more contents on 4 objects not shown
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Powerwall_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 2.2 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.22 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.183333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.157142857142857 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.1375 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Powerwall 1200x600x180_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.122222222222222 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Powerwall 1200x600x40_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.55 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Powerwall 1200x600x50_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.44 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon: 16 more contents on 4 objects not shown
  Identity Data(Type) | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Model Text 1" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "standaard" (IFCIDENTIFIER)
  Graphics | properties | on 11 objects (11 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "1200x600" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "100" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "120" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "140" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "160" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "180" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "40" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "50" (IFCTEXT)
  Graphics: 6 more contents on 5 objects not shown
  Identity Data | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Subcategory = "Generic Models" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_22_WA_Powerwall_Recticel Insulation" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "standaard" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_22_WA_Powerwall 1200x600x100_Recticel Insulation" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_22_WA_Powerwall 1200x600x120_Recticel Insulation" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_22_WA_Powerwall 1200x600x140_Recticel Insulation" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_22_WA_Powerwall 1200x600x160_Recticel Insulation" (IFCTEXT)
  Identity Data: 7 more contents on 0 objects not shown
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Text(Type) | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Bold = FALSE (IFCBOOLEAN)
    Italic = FALSE (IFCBOOLEAN)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 2.2 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.454545454545455 (IFCREAL)
    Thermal mass = 448. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.22 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 4.54545454545455 (IFCREAL)
    Thermal mass = 4480. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.183333333333333 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 5.45454545454546 (IFCREAL)
    Thermal mass = 5376. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.157142857142857 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 6.36363636363636 (IFCREAL)
    Thermal mass = 6272. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.1375 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 7.27272727272727 (IFCREAL)
    Thermal mass = 7168. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.122222222222222 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 8.18181818181818 (IFCREAL)
    Thermal mass = 8064. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.55 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 1.81818181818182 (IFCREAL)
    Thermal mass = 1792. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.44 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 2.27272727272727 (IFCREAL)
    Thermal mass = 2240. (IFCREAL)
  Analytical Properties: 4 more contents on 0 objects not shown
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 120. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 140. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 160. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 180. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 40. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 50. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction: 4 more contents on 0 objects not shown
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "BERSnl_x_rgb 0 0 0 T00 zwart_gen" (IFCLABEL)
    TBQnl_C_materiaal_02 = "BERSnl_x_rgb 255 203 012 T00 geel_gen" (IFCLABEL)

Other addresses and roles
  2 x postal address (none given)