IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2021-02-22T12:01:17"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.09 : 26 Sep 2013"
Originating system: "21.1.0.108 - Exporter 21.1.0.108 - IFC Model Exchange with Archicad 24.0.0.4000"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"
Application: "IFC Model Exchange with Archicad for Revit 2021" version "24.0.0" identifier "Add-in version: 4000 INT 64 bit" by Organization "GRAPHISOFT SE"

People and organizations
  Person "Autodesk" of Organization (no name given)
  Owner history of Person "Autodesk" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1613991203 (2021-02-22T10:53:23Z)
  Owner history of Person "Autodesk" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | created 1613991203 (2021-02-22T10:53:23Z) | last modified with "IFC Model Exchange with Archicad for Revit 2021" version "24.0.0" identifier "Add-in version: 4000 INT 64 bit" by Organization "GRAPHISOFT SE"

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 46 elements
          12 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "NLRS_XX_GM_FB_logo_recticel:standaard" | object type "NLRS_XX_GM_FB_logo_recticel:standaard" | names: "NLRS_XX_GM_FB_logo_recticel:standaard:4786", "NLRS_XX_GM_FB_logo_recticel:standaard:75714", "NLRS_XX_GM_FB_logo_recticel:standaard:75754" (+9 more) | material: materials ("NLRS_x_rgb 0 0 0 T00 zwart_gen", "NLRS_x_rgb 255 203 012 T00 geel_gen") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:4787" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCROOF | object type "Basic Roof:NLRS_27_RO_Eurothane Bi-4_Recticel Insulation" | names: "Basic Roof:NLRS_27_RO_Eurothane Bi-4_Recticel Insulation:75698" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75716" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCROOF | object type "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x100_Recticel Insulation" | names: "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x100_Recticel Insulation:75738" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75756" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75757" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCROOF | object type "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x120_Recticel Insulation" | names: "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x120_Recticel Insulation:75778" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75796" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75797" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCROOF | object type "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x140_Recticel Insulation" | names: "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x140_Recticel Insulation:75818" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75836" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75837" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCROOF | object type "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x30_Recticel Insulation" | names: "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x30_Recticel Insulation:75858" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75876" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75877" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCROOF | object type "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x40_Recticel Insulation" | names: "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x40_Recticel Insulation:75898" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75916" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75917" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCROOF | object type "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x50_Recticel Insulation" | names: "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x50_Recticel Insulation:75938" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75956" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75957" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCROOF | object type "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x60_Recticel Insulation" | names: "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x60_Recticel Insulation:75978" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75996" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75997" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCROOF | object type "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x70_Recticel Insulation" | names: "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x70_Recticel Insulation:76018" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:76036" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:76037" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCROOF | object type "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x80_Recticel Insulation" | names: "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x80_Recticel Insulation:76058" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:76076" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:76077" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCROOF | object type "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x91_Recticel Insulation" | names: "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x91_Recticel Insulation:76098" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:76116" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:76117" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:76118" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | elevation 4000.

Types
  IFCBUILDINGELEMENTPROXYTYPE "NLRS_XX_GM_FB_logo_recticel:standaard" | 12 occurrences | material: materials ("NLRS_x_rgb 255 203 012 T00 geel_gen", "NLRS_x_rgb 0 0 0 T00 zwart_gen") | property sets: Constraints, Identity Data, Materials and Finishes, Other, Pset_BuildingElementProxyCommon, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_ProductRequirements | properties | on 35 objects (35 IFCBUILDINGELEMENTPROXY) | on 24 type objects
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 22 objects (11 IFCROOF, 11 IFCSLAB)
    Category = "Roofs" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Model Text: Model Text 1" (IFCLABEL)
    Family and Type = "Model Text: Model Text 1" (IFCLABEL)
    Type = "Model Text: Model Text 1" (IFCLABEL)
    Type Id = "Model Text: Model Text 1" (IFCLABEL)
  Other | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "NLRS_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Family and Type = "NLRS_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Type = "NLRS_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Type Id = "NLRS_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family = "Basic Roof: NLRS_27_RO_Eurothane Bi-4_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Roof: NLRS_27_RO_Eurothane Bi-4_Recticel Insulation" (IFCLABEL)
    Type = "Basic Roof: NLRS_27_RO_Eurothane Bi-4_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Roof: NLRS_27_RO_Eurothane Bi-4_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x100_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x100_Recticel Insulation" (IFCLABEL)
    Type = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x100_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x100_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x120_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x120_Recticel Insulation" (IFCLABEL)
    Type = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x120_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x120_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x140_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x140_Recticel Insulation" (IFCLABEL)
    Type = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x140_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x140_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x30_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x30_Recticel Insulation" (IFCLABEL)
    Type = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x30_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Roof: NLRS_27_RO_Eurothane Bi-4 1200x600x30_Recticel Insulation" (IFCLABEL)
  Other: 9 more contents on 7 objects not shown
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY) | on 23 type objects
    Reference = "Model Text:Model Text 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "NLRS_XX_GM_FB_logo_recticel:standaard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY) | on 23 type objects
    Reference = "Model Text:Model Text 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "NLRS_XX_GM_FB_logo_recticel:standaard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x140_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x30_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x40_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 5 more contents on 10 objects not shown
  Pset_ProvisionForVoid | properties | on 22 objects (22 IFCBUILDINGELEMENTPROXY)
    Depth = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape = "Undefined" (IFCLABEL)
    Width = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 2. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 43.9375 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 2. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 75.3422326122 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape = "Undefined" (IFCLABEL)
    Width = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Work Plane = "Level : Level 1" (IFCTEXT)
  Constraints | properties | on 11 objects (11 IFCROOF)
    Base Level = "Level: Level 1" (IFCLABEL)
    Base Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Cutoff Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Schedule Level = "Level: Level 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Roof : NLRS_27_RO_Eurothane Bi-4_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Roof : NLRS_27_RO_Eurothane Bi-4 1200x600x100_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Roof : NLRS_27_RO_Eurothane Bi-4 1200x600x120_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Roof : NLRS_27_RO_Eurothane Bi-4 1200x600x140_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Roof : NLRS_27_RO_Eurothane Bi-4 1200x600x30_Recticel Insulation" (IFCTEXT)
  Constraints: 8 more contents on 7 objects not shown
  Dimensions | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Depth = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY)
    Area = 0.114476516317 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.000206579980456 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCROOF)
    Area = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.1124126784 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCROOF)
    Area = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.124126784 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCROOF)
    Area = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 120. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.3489521408 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCROOF)
    Area = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 140. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.5737774976 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCROOF)
    Area = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.3372380352 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCROOF)
    Area = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.4496507136 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 6 more contents on 6 objects not shown
  Phasing | properties | on 46 objects (35 IFCBUILDINGELEMENTPROXY, 11 IFCROOF)
    Phase Created = "New Construction" (IFCLABEL)
  Graphics | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "1200x600" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "text" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "x" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "100" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "120" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "140" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "30" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "40" (IFCTEXT)
  Graphics: 6 more contents on 6 objects not shown
  Identity Data | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Subcategory = "Generic Models" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 23 type objects
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Model Text 1" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "standaard" (IFCTEXT)
  Pset_ElementShading | properties | on 22 objects (11 IFCROOF, 11 IFCSLAB)
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x140_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x30_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x40_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x50_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x60_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon: 3 more contents on 3 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x100_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x120_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x140_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x30_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x40_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x50_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x60_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab: 3 more contents on 3 objects not shown
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 2.6 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.26 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.216666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x140_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.185714285714 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x30_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.866666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x40_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.65 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x50_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.52 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Basic Roof:NLRS_27_RO_Eurothane Bi-4 1200x600x60_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.433333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon: 3 more contents on 3 objects not shown
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 120. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 140. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 60. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction: 3 more contents on 3 objects not shown
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  AC_Pset_RenovationAndPhasing | properties | on 57 objects (35 IFCBUILDINGELEMENTPROXY, 11 IFCROOF, 11 IFCSLAB)
    Renovation Status = "New" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "NLRS_x_rgb 0 0 0 T00 zwart_gen" (IFCLABEL)
    TBQnl_C_materiaal_02 = "NLRS_x_rgb 255 203 012 T00 geel_gen" (IFCLABEL)
  Text | properties | on 23 type objects
    Bold = FALSE (IFCBOOLEAN)
    Italic = FALSE (IFCBOOLEAN)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 600. (IFCLENGTHMEASURE) [MILLI METRE]