IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2021-02-22T12:04:51"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.09 : 26 Sep 2013"
Originating system: "21.1.0.108 - Exporter 21.1.0.108 - IFC Model Exchange with Archicad 24.0.0.4000"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"
Application: "IFC Model Exchange with Archicad for Revit 2021" version "24.0.0" identifier "Add-in version: 4000 INT 64 bit" by Organization "GRAPHISOFT SE"

People and organizations
  Person "Autodesk" of Organization (no name given)
  Owner history of Person "Autodesk" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1613991235 (2021-02-22T10:53:55Z)
  Owner history of Person "Autodesk" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | created 1613991235 (2021-02-22T10:53:55Z) | last modified with "IFC Model Exchange with Archicad for Revit 2021" version "24.0.0" identifier "Add-in version: 4000 INT 64 bit" by Organization "GRAPHISOFT SE"

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 46 elements
          12 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "NLRS_XX_GM_FB_logo_recticel:standaard" | object type "NLRS_XX_GM_FB_logo_recticel:standaard" | names: "NLRS_XX_GM_FB_logo_recticel:standaard:4786", "NLRS_XX_GM_FB_logo_recticel:standaard:75694", "NLRS_XX_GM_FB_logo_recticel:standaard:75713" (+9 more) | material: materials ("NLRS_x_rgb 0 0 0 T00 zwart_gen", "NLRS_x_rgb 255 203 012 T00 geel_gen") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:4787" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75660" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro_Recticel Insulation" | object type "Basic Wall:NLRS_22_WA_Eurowall Xentro_Recticel Insulation" | names: "Basic Wall:NLRS_22_WA_Eurowall Xentro_Recticel Insulation:75661" | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro_Recticel Insulation" 10.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75697" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" | object type "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" | names: "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation:75698" | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x100_Recticel Insulation" 100.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75715" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75716" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" | object type "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" | names: "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation:75717" | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x105_Recticel Insulation" 105.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75734" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75735" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" | object type "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" | names: "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation:75736" | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x110_Recticel Insulation" 110.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75753" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75754" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" | object type "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" | names: "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation:75755" | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x120_Recticel Insulation" 120.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75772" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75773" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x30_Recticel Insulation" | object type "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x30_Recticel Insulation" | names: "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x30_Recticel Insulation:75774" | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x30_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x30_Recticel Insulation" 30.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75791" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75792" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x50_Recticel Insulation" | object type "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x50_Recticel Insulation" | names: "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x50_Recticel Insulation:75793" | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x50_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x50_Recticel Insulation" 50.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75810" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75811" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x60_Recticel Insulation" | object type "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x60_Recticel Insulation" | names: "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x60_Recticel Insulation:75812" | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x60_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x60_Recticel Insulation" 60.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75829" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75830" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x70_Recticel Insulation" | object type "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x70_Recticel Insulation" | names: "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x70_Recticel Insulation:75831" | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x70_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x70_Recticel Insulation" 70.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75848" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75849" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x80_Recticel Insulation" | object type "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x80_Recticel Insulation" | names: "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x80_Recticel Insulation:75850" | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x80_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x80_Recticel Insulation" 80.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75867" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75868" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x90_Recticel Insulation" | object type "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x90_Recticel Insulation" | names: "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x90_Recticel Insulation:75869" | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x90_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x90_Recticel Insulation" 90.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75886" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:75887" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid, Constraints, Dimensions
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | elevation 4000.

Types
  IFCBUILDINGELEMENTPROXYTYPE "NLRS_XX_GM_FB_logo_recticel:standaard" | 12 occurrences | material: materials ("NLRS_x_rgb 255 203 012 T00 geel_gen", "NLRS_x_rgb 0 0 0 T00 zwart_gen") | property sets: Constraints, Identity Data, Materials and Finishes, Other, Pset_BuildingElementProxyCommon, Pset_ProductRequirements
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro_Recticel Insulation" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x100_Recticel Insulation" 100.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x105_Recticel Insulation" 105.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x110_Recticel Insulation" 110.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x120_Recticel Insulation" 120.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x30_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x30_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x30_Recticel Insulation" 30.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x50_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x50_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x50_Recticel Insulation" 50.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x60_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x60_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x60_Recticel Insulation" 60.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x70_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x70_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x70_Recticel Insulation" 70.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x80_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x80_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x80_Recticel Insulation" 80.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x90_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x90_Recticel Insulation" ("NLRS_FME.n7_isolatie_Eurowall Xentro 1200x600x90_Recticel Insulation" 90.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:Model Text 1" | 1 occurrence | property sets: Identity Data, Other, Text, Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_ProductRequirements | properties | on 35 objects (35 IFCBUILDINGELEMENTPROXY) | on 24 type objects
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 11 objects (11 IFCWALLSTANDARDCASE) | on 11 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Model Text: Model Text 1" (IFCLABEL)
    Family and Type = "Model Text: Model Text 1" (IFCLABEL)
    Type = "Model Text: Model Text 1" (IFCLABEL)
    Type Id = "Model Text: Model Text 1" (IFCLABEL)
  Other | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "NLRS_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Family and Type = "NLRS_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Type = "NLRS_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Type Id = "NLRS_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: NLRS_22_WA_Eurowall Xentro_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: NLRS_22_WA_Eurowall Xentro_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: NLRS_22_WA_Eurowall Xentro_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: NLRS_22_WA_Eurowall Xentro_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" (IFCLABEL)
  Other: 10 more contents on 7 objects not shown
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY) | on 23 type objects
    Reference = "Model Text:Model Text 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "NLRS_XX_GM_FB_logo_recticel:standaard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY) | on 23 type objects
    Reference = "Model Text:Model Text 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "NLRS_XX_GM_FB_logo_recticel:standaard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x30_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 5 more contents on 5 objects not shown
  Pset_ProvisionForVoid | properties | on 22 objects (22 IFCBUILDINGELEMENTPROXY)
    Depth = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape = "Undefined" (IFCLABEL)
    Width = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 2. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 43.9375 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 2. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 602.737860898 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape = "Undefined" (IFCLABEL)
    Width = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Work Plane = "Level : Level 1" (IFCTEXT)
  Constraints | properties | on 11 objects (11 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Cross-Section = "Vertical" (IFCIDENTIFIER)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 4000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Schedule Level = "Level: Level 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : NLRS_22_WA_Eurowall Xentro_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" (IFCTEXT)
  Constraints: 8 more contents on 7 objects not shown
  Dimensions | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Depth = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY)
    Area = 0.114476516317 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.000206579980456 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.134112 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.34112 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.408176 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.475232 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.609344 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.402336 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 6 more contents on 6 objects not shown
  Phasing | properties | on 46 objects (35 IFCBUILDINGELEMENTPROXY, 11 IFCWALLSTANDARDCASE)
    Phase Created = "New Construction" (IFCLABEL)
  Graphics | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "1200x600" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "text" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "x" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "100" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "105" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "110" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "120" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "30" (IFCTEXT)
  Graphics: 7 more contents on 6 objects not shown
  Identity Data | properties | on 23 objects (23 IFCBUILDINGELEMENTPROXY)
    Subcategory = "Generic Models" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 23 type objects
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Model Text 1" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "standaard" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "NLRS_22_WA_Eurowall Xentro_Recticel Insulation" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" (IFCTEXT)
  Identity Data: 7 more contents on 0 objects not shown
  Structural | properties | on 11 objects (11 IFCWALLSTANDARDCASE)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 11 objects (11 IFCWALLSTANDARDCASE) | on 11 type objects
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x30_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x50_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x60_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 3 more contents on 3 objects not shown
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 1.9 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.19 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x105_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.180952380952 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x110_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.172727272727 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.158333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x30_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.633333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x50_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.38 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:NLRS_22_WA_Eurowall Xentro 1200x600x60_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.316666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon: 14 more contents on 3 objects not shown
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  AC_Pset_RenovationAndPhasing | properties | on 46 objects (35 IFCBUILDINGELEMENTPROXY, 11 IFCWALLSTANDARDCASE)
    Renovation Status = "New" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "NLRS_x_rgb 0 0 0 T00 zwart_gen" (IFCLABEL)
    TBQnl_C_materiaal_02 = "NLRS_x_rgb 255 203 012 T00 geel_gen" (IFCLABEL)
  Text | properties | on 23 type objects
    Bold = FALSE (IFCBOOLEAN)
    Italic = FALSE (IFCBOOLEAN)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 1.9 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Mass = 0.04162056192 (IFCREAL)
    Thermal Resistance (R) = 0.526315789474 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.19 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Mass = 0.4162056192 (IFCREAL)
    Thermal Resistance (R) = 5.26315789474 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.180952380952 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Mass = 0.43701590016 (IFCREAL)
    Thermal Resistance (R) = 5.52631578947 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.172727272727 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Mass = 0.45782618112 (IFCREAL)
    Thermal Resistance (R) = 5.78947368421 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.158333333333 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Mass = 0.49944674304 (IFCREAL)
    Thermal Resistance (R) = 6.31578947368 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.633333333333 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Mass = 0.12486168576 (IFCREAL)
    Thermal Resistance (R) = 1.57894736842 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.38 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Mass = 0.2081028096 (IFCREAL)
    Thermal Resistance (R) = 2.63157894737 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.316666666667 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Mass = 0.24972337152 (IFCREAL)
    Thermal Resistance (R) = 3.15789473684 (IFCREAL)
  Analytical Properties: 3 more contents on 0 objects not shown
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 105. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 110. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 120. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 50. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 60. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction: 3 more contents on 0 objects not shown