IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2020-12-23T14:16:07"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190510_1515(x64) - Exporter 18.4.0.0 - Alternate UI 18.4.0.0"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "ktemmerman" of Organization (no name given)
  Owner history of Person "ktemmerman" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 1608728403 (2020-12-23T13:00:03Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 69 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation:74944" | material: layers "Basic Wall:BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro_Recticel Insulation" 10.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          18 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "standaard" | object type "BERSnl_XX_GM_FB_logo_recticel:standaard" | names: "BERSnl_XX_GM_FB_logo_recticel:standaard:74959", "BERSnl_XX_GM_FB_logo_recticel:standaard:74978", "BERSnl_XX_GM_FB_logo_recticel:standaard:74997" (+15 more) | material: materials ("BERSnl_x_rgb 0 0 0 T00 zwart_gen", "BERSnl_x_rgb 255 203 012 T00 geel_gen") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Other
          33 x IFCBUILDINGELEMENTPROXY | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:74962", "Model Text:Model Text 1:74980", "Model Text:Model Text 1:74981" (+30 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation:74963" | material: layers "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x20_Recticel Insulation" 20.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation:74982" | material: layers "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x30_Recticel Insulation" 30.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation:75001" | material: layers "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x40_Recticel Insulation" 40.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation:75020" | material: layers "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x50_Recticel Insulation" 50.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x60_Recticel Insulation" | object type "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x60_Recticel Insulation" | names: "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x60_Recticel Insulation:75039" | material: layers "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x60_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x60_Recticel Insulation" 60.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_ElementShading
          1 x IFCSLAB | type IFCSLABTYPE "Floor:BERSnl_23_FL_Eurothane G Xentro_Recticel Insulation" | object type "Floor:BERSnl_23_FL_Eurothane G Xentro_Recticel Insulation" | FLOOR | names: "Floor:BERSnl_23_FL_Eurothane G Xentro_Recticel Insulation:78555" | material: layers "Floor:BERSnl_23_FL_Eurothane G Xentro_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro_Recticel Insulation" 10.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints
          1 x IFCSLAB | type IFCSLABTYPE "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x20_Recticel Insulation" | object type "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x20_Recticel Insulation" | FLOOR | names: "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x20_Recticel Insulation:78585" | material: layers "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x20_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x20_Recticel Insulation" 20.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints
          1 x IFCSLAB | type IFCSLABTYPE "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x30_Recticel Insulation" | object type "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x30_Recticel Insulation" | FLOOR | names: "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x30_Recticel Insulation:78615" | material: layers "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x30_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x30_Recticel Insulation" 30.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints
          1 x IFCSLAB | type IFCSLABTYPE "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x40_Recticel Insulation" | object type "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x40_Recticel Insulation" | FLOOR | names: "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x40_Recticel Insulation:78645" | material: layers "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x40_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x40_Recticel Insulation" 40.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints
          1 x IFCSLAB | type IFCSLABTYPE "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x50_Recticel Insulation" | object type "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x50_Recticel Insulation" | FLOOR | names: "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x50_Recticel Insulation:78675" | material: layers "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x50_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x50_Recticel Insulation" 50.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints
          1 x IFCSLAB | type IFCSLABTYPE "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x60_Recticel Insulation" | object type "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x60_Recticel Insulation" | FLOOR | names: "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x60_Recticel Insulation:78705" | material: layers "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x60_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x60_Recticel Insulation" 60.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Constraints
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane G Xentro_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane G Xentro_Recticel Insulation:82338" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane G Xentro 2600x1200x20_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane G Xentro 2600x1200x20_Recticel Insulation:82377" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane G Xentro 2600x1200x30_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane G Xentro 2600x1200x30_Recticel Insulation:82416" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane G Xentro 2600x1200x40_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane G Xentro 2600x1200x40_Recticel Insulation:82455" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane G Xentro 2600x1200x50_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane G Xentro 2600x1200x50_Recticel Insulation:82494" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane G Xentro 2600x1200x60_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane G Xentro 2600x1200x60_Recticel Insulation:82533" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction

Types
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro_Recticel Insulation" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCBUILDINGELEMENTPROXYTYPE "standaard" | 18 occurrences | material: materials ("BERSnl_x_rgb 0 0 0 T00 zwart_gen", "BERSnl_x_rgb 255 203 012 T00 geel_gen") | property sets: Constraints, Identity Data, Materials and Finishes, Other, Pset_BuildingElementProxyCommon, Pset_ProductRequirements
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x20_Recticel Insulation" 20.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x30_Recticel Insulation" 30.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x40_Recticel Insulation" 40.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x50_Recticel Insulation" 50.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCWALLTYPE "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x60_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSnl_22_WA_Eurothane G Xentro 2600x1200x60_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x60_Recticel Insulation" 60.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCSLABTYPE "Floor:BERSnl_23_FL_Eurothane G Xentro_Recticel Insulation" | FLOOR | 1 occurrence | material: layers "Floor:BERSnl_23_FL_Eurothane G Xentro_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro_Recticel Insulation" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCSLABTYPE "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x20_Recticel Insulation" | FLOOR | 1 occurrence | material: layers "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x20_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x20_Recticel Insulation" 20.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCSLABTYPE "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x30_Recticel Insulation" | FLOOR | 1 occurrence | material: layers "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x30_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x30_Recticel Insulation" 30.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCSLABTYPE "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x40_Recticel Insulation" | FLOOR | 1 occurrence | material: layers "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x40_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x40_Recticel Insulation" 40.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCSLABTYPE "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x50_Recticel Insulation" | FLOOR | 1 occurrence | material: layers "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x50_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x50_Recticel Insulation" 50.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCSLABTYPE "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x60_Recticel Insulation" | FLOOR | 1 occurrence | material: layers "Floor:BERSnl_23_FL_Eurothane G Xentro 2600x1200x60_Recticel Insulation" ("BERSnl_FME.n7_isolatie_Eurothane G Xentro 2600x1200x60_Recticel Insulation" 60.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading

Property sets
  Other(Type) | properties | on 33 objects (33 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Model Text" (IFCTEXT)
  Other(Type) | properties | on 6 objects (6 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family Name = "Basic Roof" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints | properties | on 33 objects (33 IFCBUILDINGELEMENTPROXY)
    Work Plane = "Level : Level 1" (IFCTEXT)
  Constraints | properties | on 6 objects (6 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 4000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 6 objects (6 IFCSLAB)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: Level 1" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 6 objects (6 IFCROOF)
    Base Level = "Level: Level 1" (IFCLABEL)
    Base Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Cutoff Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCTEXT)
  Constraints: 16 more contents on 15 objects not shown
  Dimensions | properties | on 33 objects (33 IFCBUILDINGELEMENTPROXY)
    Depth = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    Area = 0.114476516316835 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.000206579980456013 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.134111999999969 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.268223999999939 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.402335999999909 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.536447999999878 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.670559999999848 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 13.4112 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3352.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.804671999999817 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 13 more contents on 13 objects not shown
  Other | properties | on 33 objects (33 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Model Text: Model Text 1" (IFCLABEL)
    Family and Type = "Model Text: Model Text 1" (IFCLABEL)
    Type = "Model Text: Model Text 1" (IFCLABEL)
    Type Id = "Model Text: Model Text 1" (IFCLABEL)
  Other | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "BERSnl_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Family and Type = "BERSnl_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Type = "BERSnl_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Type Id = "BERSnl_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation" (IFCLABEL)
    Type = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Wall: BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation" (IFCLABEL)
  Other: 17 more contents on 14 objects not shown
  Phasing | properties | on 69 objects (51 IFCBUILDINGELEMENTPROXY, 6 IFCROOF, 6 IFCSLAB, 6 IFCWALLSTANDARDCASE)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 6 objects (6 IFCWALLSTANDARDCASE)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Structural | properties | on 6 objects (6 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Pset_ElementShading | properties | on 24 objects (12 IFCSLAB, 6 IFCROOF, 6 IFCWALLSTANDARDCASE) | on 12 type objects
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProductRequirements | properties | on 51 objects (51 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 12 objects (6 IFCROOF, 6 IFCSLAB)
    Category = "Roofs" (IFCLABEL)
  Pset_ProductRequirements | properties | on 6 objects (6 IFCWALLSTANDARDCASE) | on 6 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 6 objects (6 IFCSLAB) | on 6 type objects
    Category = "Floors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 33 objects (33 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "standaard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane G Xentro_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x50_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x60_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 12 more contents on 12 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x60_Recticel Insulation" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 1.9 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.95 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.633333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.475 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.38 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x60_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.316666666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 1.9 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.95 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon: 4 more contents on 0 objects not shown
  Identity Data(Type) | properties | on 33 objects (33 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Model Text 1" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_27_RO_Eurothane G Xentro_Recticel Insulation" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x50_Recticel Insulation" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x60_Recticel Insulation" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 33 objects (33 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "standaard" (IFCIDENTIFIER)
  Graphics | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "2600x1200" (IFCTEXT)
  Graphics | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "20" (IFCTEXT)
  Graphics | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "30" (IFCTEXT)
  Graphics | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "40" (IFCTEXT)
  Graphics | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "50" (IFCTEXT)
  Graphics | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "60" (IFCTEXT)
  Graphics | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Eurothane G Xentro" (IFCTEXT)
  Graphics | properties | on 12 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Identity Data | properties | on 33 objects (33 IFCBUILDINGELEMENTPROXY)
    Subcategory = "Generic Models" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_22_WA_Eurothane G Xentro_Recticel Insulation" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "standaard" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_22_WA_Eurothane G Xentro 2600x1200x50_Recticel Insulation" (IFCTEXT)
  Identity Data: 7 more contents on 0 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "BERSnl_23_FL_Eurothane G Xentro_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "BERSnl_23_FL_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "BERSnl_23_FL_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "BERSnl_23_FL_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "BERSnl_23_FL_Eurothane G Xentro 2600x1200x50_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "BERSnl_23_FL_Eurothane G Xentro 2600x1200x60_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane G Xentro_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab: 4 more contents on 4 objects not shown
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_23_FL_Eurothane G Xentro_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 1.9 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_23_FL_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.95 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_23_FL_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.633333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_23_FL_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.475 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_23_FL_Eurothane G Xentro 2600x1200x50_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.38 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_23_FL_Eurothane G Xentro 2600x1200x60_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.316666666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_27_RO_Eurothane G Xentro_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 1.9 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.95 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon: 10 more contents on 4 objects not shown
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane G Xentro_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x20_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x30_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x40_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x50_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane G Xentro 2600x1200x60_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 60. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 20. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction: 10 more contents on 0 objects not shown
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Text(Type) | properties | on 33 objects (33 IFCBUILDINGELEMENTPROXY)
    Bold = FALSE (IFCBOOLEAN)
    Italic = FALSE (IFCBOOLEAN)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 1.9 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.526315789473684 (IFCREAL)
    Thermal mass = 420. (IFCREAL)
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.95 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 1.05263157894737 (IFCREAL)
    Thermal mass = 840. (IFCREAL)
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.633333333333333 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 1.57894736842105 (IFCREAL)
    Thermal mass = 1260. (IFCREAL)
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.475 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 2.10526315789474 (IFCREAL)
    Thermal mass = 1680. (IFCREAL)
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.38 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 2.63157894736842 (IFCREAL)
    Thermal mass = 2100. (IFCREAL)
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.316666666666667 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 3.15789473684211 (IFCREAL)
    Thermal mass = 2520. (IFCREAL)
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 20. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 40. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 60. (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics(Type) | properties | on 6 objects (6 IFCROOF)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Analytical Properties | properties | on 2 type objects
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 1.9 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.526315789473684 (IFCREAL)
    Thermal mass = 420. (IFCREAL)
  Analytical Properties | properties | on 2 type objects
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.95 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 1.05263157894737 (IFCREAL)
    Thermal mass = 840. (IFCREAL)
  Analytical Properties | properties | on 2 type objects
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.633333333333333 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 1.57894736842105 (IFCREAL)
    Thermal mass = 1260. (IFCREAL)
  Analytical Properties | properties | on 2 type objects
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.475 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 2.10526315789474 (IFCREAL)
    Thermal mass = 1680. (IFCREAL)
  Analytical Properties | properties | on 2 type objects
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.38 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 2.63157894736842 (IFCREAL)
    Thermal mass = 2100. (IFCREAL)
  Analytical Properties | properties | on 2 type objects
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.316666666666667 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 3.15789473684211 (IFCREAL)
    Thermal mass = 2520. (IFCREAL)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "BERSnl_x_rgb 0 0 0 T00 zwart_gen" (IFCLABEL)
    TBQnl_C_materiaal_02 = "BERSnl_x_rgb 255 203 012 T00 geel_gen" (IFCLABEL)

Other addresses and roles
  2 x postal address (none given)